-------------------------------------------------------------------------
------------------------------ DWLWin -----------------------------------
-------------------------------------------------------------------------

Important : This software is protected by Copyright and the information
contained herein is confidential. Distribution, reproduction as well as 
exploitation and transmission of its contents is not allowed except if 
expressly permitted. Infringments result in damage claims.
Copyright Wavecom S.A. (c) 2001.

This product includes software developed by the University of California, 
Berkeley and its contributors.



Version History
========================
V 3.2.5 (3 October 2003)
	FIXED	: Bounds of the erased area when the download address is not 0.
	FIXED	: Workaround for a problem with Intel C3 "Sawtooth" flash devices.
	ADDED	: Support for Micron MT28C3224P 32/4 1.8V.
	ADDED 	: For faster identification, version number is added in title bar.
	CHANGED : Made splash screen less intrusive and wrote full version number 
		  (bottom left corner)
	UPDATED	: "Erase Objects" wipes Java volumes too.
	

V 3.2.4.1 (8 September 2003)
	FIXED  : DWLWin could not start under Windows 95 and Windows NT 4.


V 3.2.4 (7 July 2003)
	ADDED  : Support for Wismo 2C (Q2200) modules. Important note : 
		 Autodetection does not work for these modules.
		 Select "Wismo 2C" in the "Advanced" window before 
		 downloading in this kind of module.
	ADDED  : Support for Toshiba TH50VSF1480 (16/2) devices for Wismo 2C.
	ADDED  : The baseband in Wismo P5 modules is now automatically powered 
		 up by the downloader. With some broken handsets, the user has 
		 to keep pressing the ON key during the whole download process ;
		 the key can now be safely released once the downloader starts
		 (i.e. DwlWin is connected).
	FIXED  : Improved upload (so that it does not finish before the normal 
		 end).
		 
		
V 3.2.3 (20 June 2003)
	ADDED  : Path can be typed or pasted in "Working Dir" edit box.
	ADDED  : Full path is displayed in "Working Dir" browse dialog box.
	FIXED  : DWLWin could not start under Windows 95.
	CHANGED: The key in .ini file now disables "FLASH" and "External RAM"
		 buttons in "Download Place".
	

V 3.2.2 (13 June 2003)
	FIXED  : Make sure "Working Dir" path is always in long format (sometimes
		 was in 8.3 old DOS format before).
	FIXED  : Always unchecks "Erase Wavecom Binary" button when changing 
		 "Working Dir" path.
	ADDED  : A key in .ini file to disable RAM radio buttons in "Download 
		 Place".
	ADDED  : Support for more flash devices.
		 For Qx/P3 : 
		 	TOSHIBA TH50VSF2582, 32 Mb ROM 4 Mb RAM (mass produced
		 	devices were not recognized before)
		 For P5 : 
		 	INTEL 28F320W18, 32 Mb ROM 4 Mb RAM
		 	ST M36DR864TB, 64 Mb ROM 4/8 Mb RAM
		 

V 3.2.1 (22 May 2003)
	FIXED  : Customization files download problems.
	FIXED  : Downloader initialisation error when the previous process
		 was interrupted.


V 3.2 (14 May 2003)

	FIXED:   The boot sequence for Wismo 5 modules is corrected. In
	         previous versions of DwlWin, selecting "Autodetect" in 
	         the CPU type list was more likely to power up a Wismo 5
	         in download mode than selecting "Wismo 5".

	CHANGED: The download sequence has been altered, in order to 
	         send EEPROM files right after the erase sequence. 
		 This should for instance prevent situations where the
		 module could download a too large customisation file
		 because the object space was configured by the eeprom
		 files received afterwards.

	CHANGED: The flash device driver has been entirely rewritten.
		 Here is the comprehensive list of the supported devices.
		 For Qx/P3 :
			INTEL 28F160C3, 16 Mb ROM / 4 Mb RAM
			INTEL 28F320C3, 32 Mb ROM / 4 Mb RAM
			ST M36W216T, 16 Mb ROM / 4 Mb RAM
			ST M36W432T, 32 Mb ROM / 4 Mb RAM
			ST M36W864TE, 64 Mb ROM / 8 Mb RAM
			TOSHIBA TH50VSF2582BESB, 32 Mb ROM / 4 Mb RAM
			TOSHIBA TH50VSF2682BFSB, 64 Mb ROM / 4-8 Mb RAM

		For P5 :
			INTEL 28F640W18, 64 Mb ROM / 4 Mb RAM
			ST M36DR432A, 32 Mb ROM / 4 Mb RAM
			TOSHIBA TH50YSF2582BFSB, 32 Mb ROM / 4 Mb RAM
			TOSHIBA TH50YSF3682AFSB, 64 Mb ROM / 8 Mb RAM

	ADDED:  Support for customisation files for products with Open MMI
	        Pack 3 and later. 
	        Note: This version can still be used to download
	        customisation files for older products; the way the .cus
	        files are stored depends on the presence and the contents
	        of an 8-bytes header.
	
	UPDATED: More precise error returns through DDE link (impacted : 
		 download start and WPB files related errors).     
	
	UPDATED: Help.


V 3.1.5 (8 April 2003)
	ADDED : Capability to download several .wpb files
	ADDED : Toshiba 64/8 devices support.
	ADDED : .wpb files selection forbidden if download in RAM ("Advanced"
		 thumb)
	
	
V 3.1.4 (26 March 2003)
	UPDATED : DDE command "SetOptions" now supports download start address.


V 3.1.3 (3 March 2003)
	ADDED : Several instances of DWLWin may be DDE-driven by several 
		instances of client software.
	ADDED : INTEL GE28F640W18 device support.
	ADDED : Wismo Q31xx support.
		  

V 3.1.2 (21 January 2003)
	UPDATED : DDE command "SetOptions" now supports several .e2p and
		  .cus files.
	UPDATED : Dongle handler. Dongle is scanned when DWLWin starts,
		  not when selecting "Advanced" thumb.
	          IMPORTANT : if you are using a local dongle, you need
		  to update the dongle driver (V 5.41)
	UPDATED : Port scanning scheme ("Port Number" on "Download" thumb)
		  Under Windows 9x port numbers always range from 1 to 16.
		  Under NT-kernel-based Windows, serial ports are scanned
		  (only actually present port numbers are displayed).
		

V 3.1.1.1 (19 December 2002)
	FIXED : Crash on Windows 9x, the 10 first seconds of the
		process, when battery is low or target sensible.
		Note : On Windows 9x, DWLWin is roughly 4 % slower
		than on NT-kernel-based Windows versions (NT / 2000 / XP).
	

V 3.1.1 (4 December 2002)
	ADDED : "CPU type" may be configured by DDE link.


V 3.1.0.0 (15 November 2002)
	ADDED   : Binary file may be downloaded in internal AND external RAM.
	ADDED	: wpb extension in "General" thumb.
	ADDED	: Possibility to "browse" thumbs during a download.
	UPDATED : Help for wpb files.


V 3.0.2.0 (31 October 2002)
	FIXED	: Initlock files bug with Toshiba flash devices.
	UPDATED : Help.


V 3.0.1.0 (25 October 2002)
	FIXED	: Communication problems between DWLWin and remote DDE clients.
	CHANGED : Program installer.


V 3.0.0.0 (18 October 2002)
	ADDED	: Wavecom Packed Binary (.wpb) files support.
		  These files are compressed binary files that allow faster 
		  downloads.
	ADDED 	: WISMO5/P5186 support.
	ADDED   : Selection of internal CPU depending on WISMO version.
 		  EXPERIMENTAL : An "Autodetect" (not suitable yet for handsets)
		  tries to determine the internal CPU type.
	ADDED	: Checks version consistency between DWLWin and downloader.
	ADDED	: Toshiba TH50VSF2582/2682, ST M36DR432/864 and 
		  Micron MT28C3224P18 devices support.
	ADDED	: Warnings on various potentially hazardous selections in
		  "Advanced" thumb.
	FIXED 	: Bug on previous version : parameters were not saved while
		  quitting DWLWin.
	FIXED	: Occasional wrong parsings/downloads of EEPROM parameters
		  (e.g. while erasing whole flash).


V 2.9.14.0 (4 September 2002)
        NEW	: GPRS Class 10 compliant modules supported.
	FIXED	: No need to append "new line" and "carriage return" characters
		  at the end of an .e2p file.


V 2.9.13.0 (26 July 2002)
	UPDATED	: Help for file associations (see "General").
	ADDED 	: When a error on a dongle occurs, DWLWin displays an error 
		  dialog box.
	ADDED 	: A DDE command permitting to abort a download.


V 2.9.12.0 (2 July 2002)
	FIXED	: Wrong working directory sometimes displayed on DWLWin startup.
	FIXED	: Wrong serial port selected on DWLWin startup (when more than 9
		  serial ports).
	CHANGED : The DDE command to set download options : Options are now serial
		  port-specific (they are not global to all ports)
	CHANGED : When selecting "AutoStart" and "AutoQuit" (in "General" thumb);
		  DWLWin will not quit now if you click on "Abort".
	CHANGED : Beep frequency.
	ADDED	: File associations (see "General" thumb). Files whose length is 
		  greater than 8 characters will not be checked in list boxes.
	ADDED	: Help button.
	ADDED	: The name of file currently downloaded (.bin or .cus) is displayed.
	ADDED	: A DDE command permitting to get flash informations (size and type).
	

V 2.9.11.0 (23 April 2002)
	CHANGED : Help redesigned for Muse (Open MMI).


V 2.9.10.0 (5 April 2002)
	CHANGED : Automatic internal reboot after process completion unless 
                  "Reset after download" is checked : no more need to reset 
                  the target between two processes.
        CHANGED : Small speed improvment.
	CHANGED	: New lock initialisation scheme (INCOMPATIBLE with the 
                  current softwares on Toshiba flash devices; fully compatible 
                  with all recent softwares on ST or Intel devices, the list 
                  of the incompatible old softwares is beyond the scope of this 
                  document).
	ADDED	: Support for serial link speeds higher than 115200 bps
                  (if the hardware supports them).


V 2.9.6.0 (27 February 2002)
	FIXED	: Upload, now much more reliable.
	CHANGED	: Timeouts, to enhance reliability on non-powerful PCs
		  (downloads were sometimes suddenly stopped).
	ADDED	: Acknoledgement for "download over" DDE frames.


V 2.9.3.0 (15 February 2002)
	FIXED	: Various minor bugs on customization files download.
	CHANGED	: DDE link updated to support customization files.
	CHANGED	: Help updated.
	

V 2.9.0.0 (7 February 2002)
	ADDED 	: A customization files (.cus) selector allowing to download
		  the corresponding files onto the target.
	ADDED	: A "Customization Files" erase check box.
	CHANGED	: Progress bar moves and sector number are displayed while
		  erasing FLASH.
	CHANGED : The "Objects" erase check box may be checked without selecting
		  a binary file. This option only erases objects in flash, not 
		  also the Wavecom binary, as before.
 

V 2.8.0.0 (18 January 2002)
	FIXED	: Various problems on download (flash size, Wismo type,...).
	ADDED	: Tooltips when pointing .bin or .e2p file.
	ADDED	: Directory for upload file.
	CHANGED	: Download start address was moved to "Advanced" page.
	

V 2.7.6.0 (2 January 2002)
	FIXED	: Bugs on download.
	FIXED   : DDE frames emission (waits 200 ms between two emissions).


V 2.7.2.0 (27 November 2001)
	FIXED   : When a path was kept in combo-box and selected in the 
		  directory dialog box, it was not taken into account.
	CHANGED : DWLWin does not delete heading space(s) in EEPROM 
		  parameters anymore.


V 2.7.0.0 (14 November 2001)
	FIXED   : download of EEPROM parameters. Some parameters were
                  sometimes not effectively downloaded.
	CHANGED : Enhanced precision of file size display in Download page.
	ADDED   : a combo-box for the Working Directory, allowing to keep 
                  the five last selected paths.
	ADDED   : several EEPROM parameters files may now be downloaded.
	ADDED   : an advanced option : "Do not send terminal data".


V 2.5.0.0 (6 July 2001)
	Fully functionnal port of DWLPC.

