-------------------------------------------------------------------------
------------------------------ DWLWin -----------------------------------
-------------------------------------------------------------------------

Important : This software is protected by Copyright and the information
contained herein is confidential. Distribution, reproduction as well as 
exploitation and transmission of its contents is not allowed except if 
expressly permitted. Infringments result in damage claims.
Copyright Sierra Wireless (c) 2009

This product includes software developed by the University of California, 
Berkeley and its contributors.

   ----------------------------------------------------------------------

Changelog:
----------
Version 4.1.6.16 (2009-11-20):
	FIXED: Production issues related to the new Numonyx RAM

Version 4.1.6.15 (2009-08-28):
	UPDATED: Wavecom is now a Sierra Wireless brand
	FIXED: Production bench issue in SWI factory (memory information)

Version 4.1.6.14 (2009-03-24):
	FIXED: Improved recovery when the download is interrupted by a power loss

Version 4.1.6.13 (2009-03-03):
        FIXED: COM function isBootOK returns TRUE although no HW info available

Version 4.1.6.12 (2009-02-26):
        UPDATED: WMP100 customers'dongles never expire

Version 4.1.6.11 (2008-12-17):
        FIXED: Serial connection issues encountered on Wavecom download benches

Version 4.1.6.10 (2008-11-17):
        FIXED: Some serial connection issues during downloads
        FIXED: Weird CPU type selection changes

Version 4.1.6.9 (2008-07-31):
        FIXED: Production issues with Q39 and Q64 processors
        ADDED: Enhancements for preprogrammed flash devices image

Version 4.1.6.8 (2008-07-21):
        FIXED: Maintenance (Wavecom internal purposes)

Version 4.1.6.7 (2008-06-20):
        FIXED: WMP50 support

Version 4.1.6.6 (2008-04-30):
        FIXED: Internal functions used in WPK files (Q2686 issue)

Version 4.1.6.5 (2008-03-25):
        UPDATED: Flash memory driver (IDS related enhancements)

Version 4.1.6.4 (2008-03-03):
        UPDATED: Flash memory driver (IDS related enhancements)
        ADDED: Support for WPB files with improved compression
        FIXED: TMT awareness

Version 4.1.6.3 (2008-01-25):
        FIXED: Secure Data Storage initialisation w/ Erase whole flash

Version 4.1.6.2 (2008-01-22):
        FIXED: Production issues with WMP processors

Version 4.1.6.1 (2008-01-13):
        FIXED: Early support for 128K bootloaders (instead of 64K)
        FIXED: Firmware erased with last OASIS2 firmware beta versions

Version 4.1.6.0 (2007-11-06):
        FIXED: EEPROM download errors with Q24 modules and OASiS 2 firmware
        UPDATED: Flash memory driver (now compatible with recent 30 nm ST parts)

Version 4.1.5.3 (2007-05-02):
        FIXED: RAM download issues
        FIXED: Trace reporting issues

Version 4.1.5.2 (2007-03-21):
        FIXED: Dropdown menus problems with Windows 2000

Version 4.1.5.1 (2007-03-09):
        ADDED: Package information through balloon tips in Download tab.

Version 4.1.5 (2007-03-06):
        ADDED: Support for WMP50
        ADDED: OLE server auto exit
        ADDED: Extra files download when a package is used
        ADDED: Multiple EEPROM files download with the command-line interface
        FIXED: Tray icon removal on OLE server exit
        FIXED: Download for Q26 Ultra
        FIXED: Upload for Q26 Ultra
        FIXED: OLE server crash on exit
        FIXED: Dongle issues

Version 4.1.4 (2007-01-30):
        FIXED: Download in internal/external RAM
        ADDED: Simple messaging from DwlWin to OLE client
        ADDED: Firmware in flash memory recognition test
        ADDED: Internal features for package support

Version 4.1.3 (2006-11-24):
        FIXED: Integer options incorrectly transmitted
        FIXED: CPU selection modified when download tab unselected
        FIXED: OLE connection crashes DwlWin when running in GUI mode

Version 4.1.2.1 (2006-11-17):
        FIXED: Internal features for package support

Version 4.1.2 (2006-11-13):
        REMOVED: Reset after download feature 
                (useless and ineffective with recent firmware versions)
        FIXED: Internal bugs
        FIXED: Wavecom products naming issues
        ADDED: Internal features in package files support

Version 4.1.1 (2006-07-28):
        ADDED: Support for flash SST 34HF3244 (32/4 combo)

Version 4.1.0.1 (2006-07-05):
        FIXED: External RAM download for Quadrium
        FIXED: Initialisation of AD volumes access through plugin API.

Version 4.1.0 (2006-06-30):
        FIXED: Downloading OS 6.60 or 6.61 beta would wrongly
               initialise the customisation files storage area and thus
               prevented upgrades from working correctly without an eeprom
               file resetting this area.
        FIXED: Failed to download PCD software before Pack3.
        ADDED: Now supports Q24-NG.
        ADDED: Early Quadrium support (will be improved in future versions).
        ADDED: WPK package files support.

Version 4.0.2 (2005-12-21):
        FIXED: Errors during download of some .e2p files
               (esp. with radio related parameters)
        FIXED: Atmel AT52BR1664AT/AT52BR3224AT support.
        FIXED: Plain downloads following downloads in waiting mode
               no longer hang unexpectedly.
        FIXED: OS 6.60 beta freezes after an erase of the Open ATŪ application. 
        ADDED: Support of WPB files created by wzpacker 1.3
               (higher compression ratios)
        ADDED: New "TMT awareness" option
               (removes the hassle of closing/reopening TMT serial port)
        ADDED: Additional copies of initlock files delivered for
               manufacturing benches.

Version 4.0.1.1 (2005-10-25):
        FIXED:  Download initialisation problems occuring with the 
                previous version.
        ADDED:  Support for flash SST 34HF1622C (16/2 combo)

Version 4.0.1 (2005-10-14):
        First released version.
        Setup bugfixes. 

Version 4.0.0 (2005-10-03):
        Initial version of DwlWin 4.


   ----------------------------------------------------------------------

Supported modules:
------------------

- Wismo 2C
- Q2303 (Wismo 2C2)
- Q2403
- P3203
- P5186
- Flex
- Q2406
- Q2686
- Q2687

Supported flash devices:
------------------------

For Q23/P32/Q24:
- Intel 28F160C3, 16 Mib ROM / 2 Mib RAM
- Intel 28F320C3, 32 Mib ROM / 4 Mib RAM
- ST M36W216T, 16 Mib ROM / 2 Mib RAM
- ST M36W432T, 32 Mib ROM / 4 Mib RAM
- ST M36W864TE, 64 Mib ROM / 8 Mib RAM
- Toshiba TH50VSF2582BESB, 32 Mib ROM / 4 Mib RAM
- Toshiba TH50VSF2682BFSB, 64 Mib ROM / 4-8 Mib RAM
- Toshiba TH50VSF1480AASB-ABSB, 16 Mib ROM / 2 Mib RAM
- Atmel AT52BR1664AT, 16 Mib ROM / 4 Mib RAM
- Atmel AT52BR3224AT, 32 Mib ROM / 4 Mib RAM
- SST 34HF1622C, 16 Mib ROM / 2 Mib RAM
- SST 34HF3244C, 32 Mib ROM / 4 Mib RAM

For Q2686/Q2687
- ST M36W0R50x0T, 32 Mib ROM / X Mib RAM
- ST M36W0R60x0T, 64 Mib ROM / X Mib RAM

For P51/Flex:
- Intel 28F320W18, 32 Mib ROM / 4 Mib RAM
- Intel 28F640W18, 64 Mib ROM / X Mib RAM
- Micron MT28C3224P, 32 Mib ROM / 4 Mib RAM
- Micron MT28C64416W18A, 64 Mib ROM /16 Mib RAM
- ST M36DR432A, 32 Mib ROM / 4 Mib RAM
- ST M36DR864TB 64 Mib ROM / 4 Mib RAM
- Toshiba TH50YSF2582BFSB, 32 Mib ROM / 4 Mib RAM       
- Toshiba TH50YSF3682AFSB, 64 Mib ROM / 8 Mib RAM       
- ST M30W0R700xT, 128 Mib ROM / X Mib RAM
- NAND Flash Samsung K9F2816Q0B 
- NAND Flash Samsung K9F2816U0B
- NAND Flash Samsung K9F5616Q0B
- NAND Flash Samsung K9F5616U0B
- NAND Flash Samsung K9F2808Q0B
- NAND Flash Samsung K9F2808U0B
- NAND Flash Samsung K9F5608Q0B
- NAND Flash Samsung K9F5608U0B
- NAND Flash Toshiba TC58DxM72A1
- NAND Flash Toshiba TC58DxM82A1
- NAND Flash Toshiba TC58DxM72A1
- NAND Flash Toshiba TC58DxM82A1
- AND Flash Renesas HN29A128A0A
- AND Flash Renesas HN29A128A1A
- AND Flash Renesas HN29V128A0A
- AND Flash Renesas HN29V128A1A



